{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","48","48","","50","50"]
["","Rafraîchissement","","Nom.","dBA","47","47","","48","48"]
["Accessoires standard","Manuel d'installation","","","","1","1","","1","1"]
["","Sachet de vis","","","","1","1","","1","1"]
["","Bouchon d'évacuation","","","","1","1","","1","1"]
["Réfrigérant","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","PRP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","kg","1.20","1.20","","1.60","1.60"]
["","Type","","","","R-410A","R-410A","","R-410A","R-410A"]
["Piping connections","Dénivelé","UI - UI","Max.","m","7.5","7.5","","7.5","7.5"]
["","","UI - UE","Max.","m","15","15","","15","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)","","0,02 (pour longueur de tuyauterie supérieure à 20 m)","0,02 (pour longueur de tuyauterie supérieure à 20 m)"]
["","Longueur totale de tuyauterie","Système","Réel","m","30","30","","30","30"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","765","765","","765","765"]
["","","","Profondeur","mm","285","285","","285","285"]
["","","","Hauteur","mm","550","550","","550","550"]
["Poids","Unité","","","kg","38","38","","42","42"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Fréquence","","","Hz","50","50","","50","50"]
["","Tension","","","V","220-240","220-240","","220-240","220-240"]
["Remarques","","","","","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés.","","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","","","550","","","550"]
["","","","Largeur","mm","","","765","","","765"]
["","","","Profondeur","mm","","","285","","","285"]
["Poids","Unité","","","kg","","","38","","","42"]
["Compresseur","Type","","","","","","Compresseur swing hermétique","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","","","10","","","10"]
["","","","Max.","°CBS","","","46","","","46"]
["","Chauffage","Temp. ambiante","Min.","°CBH","","","-15","","","-15"]
["","","","Max.","°CBH","","","15.5","","","15.5"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","","47","","","48"]
["","Chauffage","","Nom.","dBA","","","48","","","50"]
["Réfrigérant","Type","","","","","","R-410A","","","R-410A"]
["","Charge","","","kg","","","1.20","","","1.60"]
["","Charge","","","tCO2Eq","","","2.5","","","3.3"]
["","PRP","","","","","","2087.5","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","","","20","","","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","","0,02 (pour longueur de tuyauterie supérieure à 20 m)","","","0,02 (pour longueur de tuyauterie supérieure à 20 m)"]
["","Dénivelé","UI - UE","Max.","m","","","15","","","15"]
["","","UI - UI","Max.","m","","","7.5","","","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","","","30","","","30"]
["Accessoires standard","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Alimentation électrique","Phase","","","","","","1~","","","1~"]
["","Fréquence","","","Hz","","","50","","","50"]
["","Tension","","","V","","","220-240","","","220-240"]
["Accessoires standard","Réducteur","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]