{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Dimensions","Unité","","Hauteur","mm","734","734"]
["","","","Largeur","mm","1040","1040"]
["","","","Profondeur","mm","408","408"]
["Poids","Unité","","","kg","69","73"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","46","46"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48","52"]
["","Chauffage","","Nom.","dBA","49","53"]
["Réfrigérant","Type","","","","R-32","R-32"]
["","Charge","","","kg","2","2.4"]
["","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","1.35","1.62"]
["","PRP","","","","675","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","25 (2)","25 (3)"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","15 (3)","15"]
["","","UI - UI","Max.","m","7.5 (3)","7.5 (3)"]
["","Longueur totale de tuyauterie","Système","Réel","m","60","75"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Classe d'efficacité énergétique","","","","","A+++ ~ D","A+++ ~ D"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","220-440","220-240"]
["Remarques","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(2) - Par pièce","(2) - Par pièce"]
["","","","","","(3) - Pour une pièce (pour les combinaisons avec FBA71/100/125 et EKHWET et CKHWS, se reporter au manuel d'installation)","(3) - Pour une pièce (pour les combinaisons avec FBA71/100/125 et EKHWET et CKHWS, se reporter au manuel d'installation)"]
["","","","","","(4) - Contient des gaz à effet de serre fluorés.","(4) - Contient des gaz à effet de serre fluorés."]