{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Dimensions","Unité","","Hauteur","mm","734","734"]
["","","","Largeur","mm","1040","1040"]
["","","","Profondeur","mm","408","408"]
["Poids","Unité","","","kg","69.0","73.0"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","50","50"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48.0 (2)","52.0 (2)"]
["","Chauffage","","Nom.","dBA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Réfrigérant","Type","","","","R-32","R-32"]
["","Charge","","","kg","2.00","2.40"]
["","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","1.35","1.62"]
["","PRP","","","","675","675.0"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","25 (4) (5)","25 (5) (4)"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","15.0 (5)","15.0 (5)"]
["","","UI - UI","Max.","m","7.5 (5)","7.5 (5)"]
["","Longueur totale de tuyauterie","Système","Réel","m","60","75"]
["Accessoires standard","Manuel d'installation","","","","1","1"]
["","Bouchon d’évacuation","","","","3","3"]
["","Bouchon d'évacuation","","","","1","1"]
["","Réducteur","","","","1","1"]
["","Sachet de vis","","","","2","2"]
["Classe d'efficacité énergétique","","","","","A+++ ~ D","A+++ ~ D"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","220-240","220-240"]
["Remarques","","","","","(1) - Voir les schémas séparés pour la plage de fonctionnement","(1) - Voir les schémas séparés pour la plage de fonctionnement"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - Par pièce","(4) - Par pièce"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Contient des gaz à effet de serre fluorés.","(6) - Contient des gaz à effet de serre fluorés."]