{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Puissance frigorifique","Nom.","","kW","9.5","12.1 (1)"]
["Rafraîchissement des locaux","SEER","","","4.65","4.68"]
["","Consommation d’énergie annuelle","","kWh/a","716","1,550"]
["","Puissance","Pdesign","kW","9.50","12.1"]
["","Classe d’efficacité énergétique","","","B"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Classe d’efficacité énergétique","","","A"]
["","Consommation d’énergie annuelle","","kWh/a","2,498","3,340"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","D"]
["","","Chauffage","","B"]
["Puissance calorifique","Nom.","","kW","10.8","13.5 (2)"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","(2) - La consommation énergétique annuelle est conforme à la directive 2002/31/CE sur l'étiquetage énergétique.","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]
["","","","","(3) - Les valeurs SEER et SCOP sont conformes à la norme EN 14825.","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(4) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]