{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":11,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","37","37","31"]
["","","","Moyen","dBA","34","34","28"]
["","","","Bas","dBA","29","29","25"]
["","Rafraîchissement","","Moyen","dBA","32","32","28"]
["","","","Bas","dBA","29","29","25"]
["","","","Haut","dBA","35","35","30"]
["Accessoires standard","Manuel d’utilisation","","","","1","1","1"]
["","Manuel d'installation","","","","1","1","1"]
["","Flexible d'évacuation","","","","1","1","1"]
["","Bride métallique pour flexible d'évacuation","","","","1","1","1"]
["","Rondelle pour attache de suspension","","","","8","8","8"]
["","Vis","","","","40","40","40"]
["","Isolant pour raccord","","","","2","2","2"]
["","Tampons d’étanchéité","","","","5","5","5"]
["","Attaches","","","","4","4","4"]
["Systèmes de contrôle","Wired remote control","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.52","12.70","12.70"]
["","Evacuation","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60","60","56"]
["Dimensions","Unité","","Largeur","mm","700","700","1,000"]
["","","","Profondeur","mm","800","800","800"]
["","","","Hauteur","mm","245","245","245"]
["Caisson","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["","Couleur","","","","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)"]
["Poids","Unité","","","kg","28.0","28.0","35.0"]
["Ventilateur","Pression statique externe","","Haute","Pa","150","150","150"]
["","","","Nom.","Pa","30","30","30"]
["","Débit d'air","Chauffage","Haut","m³/min","15.0","15.0","18.0"]
["","","","Bas","m³/min","10.5","10.5","12.5"]
["","","","Moyen","m³/min","12.5","12.5","15.0"]
["","","Rafraîchissement","Bas","m³/min","10.5","10.5","12.5"]
["","","","Moyen","m³/min","12.5","12.5","15.0"]
["","","","Haut","m³/min","15.0","15.0","18.0"]
["Hauteur manométrique","mm","","","","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","220-240/220","220-240/220","220-240/220"]
["Remarques","","","","","(1) - Le niveau de puissance sonore est une valeur absolue générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue générée par une source sonore."]
["","","","","","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé."]
["Ventilateur","Pression statique externe","","Haute","Pa","","","","150","150","150"]
["Caisson","Couleur","","","","","","","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)"]
["","Matériau","","","","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","","","","245","245","245"]
["","","","Largeur","mm","","","","1000","1400","1400"]
["","","","Profondeur","mm","","","","800","800","800"]
["Poids","Unité","","","kg","","","","35","46","46"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","","","18","29","34"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","","","15","26","29"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","","","12.5","23","23.5"]
["","","Chauffage","Haut","m³/min","","","","18","29","34"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","","","15","26","29"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","","","12.5","23","23.5"]
["","Pression statique externe","","Nom.","Pa","","","","30","40","50"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","","","56","58","62"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","","","30","34","37"]
["","Refroidissement","","Moyen","dBA","","","","28","32","35"]
["","","","Bas","dBA","","","","25","30","32"]
["","Chauffage","","Haut","dBA","","","","31","36","38"]
["","","","Moyen","dBA","","","","28","33","35"]
["","","","Bas","dBA","","","","25","30","32"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","","9.52","9.52","9.52"]
["","Gaz","","DE","mm","","","","15.9","15.9","15.9"]
["","Évacuation","","","","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Hauteur manométrique","mm","","","","","","","625","625","625"]
["Systèmes de commande","Télécommande infrarouge","","","","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Télécommande câblée","","","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accessoires standard","Installation manual","","","","","","","1","1","1"]
["","Washer for hanger bracket","","","","","","","8","8","8"]
["","Operation manual","","","","","","","1","1","1"]
["","Clamps","","","","","","","4","4","4"]
["","Drain hose","","","","","","","1","1","1"]
["","Insulation for fitting","","","","","","","2","2","2"]
["","Metal clamp for drain hose","","","","","","","1","1","1"]
["","Screws","","","","","","","40","40","40"]
["","Sealing pads","","","","","","","5","5","5"]
["Alimentation électrique","Phase","","","","","","","1~","1~","1~"]
["","Fréquence","","","Hz","","","","50","50","50"]
["","Tension","","","V","","","","220-240/220","220-240/220","220-240/220"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","","","","","","14.00"]
["Puissance calorifique","Puissance totale","","Nom.","kW","","","","","","13.50"]