{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Niveau de pression sonore","Chauffage","Haut","dBA","37","37","31","31","36","38"]
["","","Nom.","dBA","37","37","31","31","36","38"]
["","","Moyen","dBA","34","34","28","28","33","35"]
["","","Bas","dBA","29","29","25","25","30","32"]
["","Rafraîchissement","Moyen","dBA","32","32","28","28","32","35"]
["","","Bas","dBA","29","29","25","25","30","32"]
["","","Haut","dBA","35","35","30","30","34","37"]
["","","Nom.","dBA","35","35","30","30","34","37"]
["Accessoires standard","Manuel d’utilisation","","","1","1","1","1","1","1"]
["","Manuel d'installation","","","1","1","1","1","1","1"]
["","Flexible d'évacuation","","","1","1","1","1","1","1"]
["","Bride métallique pour flexible d'évacuation","","","1","1","1","1","1","1"]
["","Rondelle pour attache de suspension","","","8","8","8","8","8","8"]
["","Vis","","","40","40","40","40","40","40"]
["","Isolant pour raccord","","","2","2","2","2","2","2"]
["","Tampon d’étanchéité","","","5","5","5","5","5","5"]
["","Attaches","","","4","4","4","4","4","4"]
["Réfrigérant","PRP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Puissance frigorifique","Puissance totale","Nom.","kW","","","","","","12.10"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gaz","DE","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Evacuation","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","60","60","56","56","58","62"]
["Dimensions","Unité","Largeur","mm","700","700","1,000","1,000","1,400","1,400"]
["","","Profondeur","mm","800","800","800","800","800","800"]
["","","Hauteur","mm","245","245","245","245","245","245"]
["Caisson","Matériau","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["","Couleur","","","Non peint","Non peint","Non peint","Non peint","Non peint","Non peint"]
["Poids","Unité","","kg","28.0","28.0","35.0","35","46","46"]
["Ventil.","Pression statique externe","Haute","Pa","150","150","150","150","150","150"]
["","","Nom.","Pa","30","30","30","30","40","50"]
["Puissance calorifique","Puissance totale","Nom.","kW","","","","","","13.5"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","Hz","50","50","50","50","50","50"]
["","Tension","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Remarques","","","","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]