{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":9,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.106","0.149"]
["","Rafraîchissement","","Nom.","kW","0.106","0.149"]
["Ventilateur","Pression statique externe","","Haute","Pa","0","0","0","0"]
["","","","Basse","Pa","0","0","0","0"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","","","12.10","13.00"]
["Puissance calorifique","Puissance totale","","Nom.","kW","","","13.5","15.5"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc"]
["","Matériau","","","","Acier galvanisé","Acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","260","260","260","285"]
["","","","Largeur","mm","1320","1538","1790","1900"]
["","","","Profondeur","mm","634","634","634","680"]
["Poids","Unité","","","kg","38","45","65","70"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","31","39"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","","31","39"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","18.9","24.8","27.2","28.3"]
["","","Chauffage","Haut","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","30.6","39.1"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","","30.6","39.1"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","18.9","24.8","27.2","28.3"]
["","Pression statique externe","","Nom.","Pa","0","0","0","0"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","59","64","65","71"]
["","Chauffage","","","dBA","62","64","65","71"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["","Refroidissement","","Moyen","dBA","","","50","53"]
["","","","Bas","dBA","46","46","49","46"]
["","Chauffage","","Haut","dBA","49","52","52","56"]
["","","","Moyen","dBA","","","50","53"]
["","","","Nom.","dBA","48","47"]
["","","","Bas","dBA","46","46","49","46"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","9.52","9.52","9.52"]
["","Gaz","","DE","mm","15.88","15.88","15.9","15.9"]
["","Évacuation","","","","19.05","19.05"]
["Systèmes de commande","Télécommande infrarouge","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Télécommande câblée","","","","ARCWB","ARCWB"]
["Accessoires standard","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Tuyau d'évacuation","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Alimentation électrique","Nom","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","220-240","220-240"]