{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","48"]
["","","","Bas","dBA","","45"]
["Accessoires standard","1","","","","","550"]
["Réfrigérant","Charge","","","kg","","2.5"]
["","Type","","","","","1.2"]
["Ventil.","Débit d'air","Rafraîchissement","Extra lent","m³/min","","30.1"]
["","","","Extra lent","cfm","","1,063"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","","740"]
["","","Chauffage","Extra lent","tr/min","","-15"]
["Plage de fonctionnement","Chauffage","Temp. ambiante","Min.","°CBH","","20"]
["","","","Max.","°CBH","","10"]
["Niveau de pression sonore","Rafraîchissement","","Bas","dBA","","44"]
["","","","Haut","dBA","","48"]
["Compresseur","Type","","","","","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","","285"]
["","","","Profondeur","mm","","612"]
["","","","Hauteur","mm","","765"]
["Poids","Unité","","","kg","","34"]
["Ventil.","Débit d'air","Chauffage","Extra lent","cfm","","904"]
["","","","Extra lent","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Tension","","","V","","220-240"]
["Remarques","","","","","(1) - 220V","(1) - Contient des gaz à effet de serre fluorés."]
["","","","","","(2) - 230 V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230 V"]
["","","","","","","(4) - 240V"]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","30.1"]
["","","Chauffage","Extra lent","m³/min","25.6"]
["","","","Extra lent","cfm","1063"]
["","","Chauffage","Extra lent","cfm","904"]
["Dimensions","Unité","","Hauteur","mm","550"]
["","","","Largeur","mm","765"]
["","","","Profondeur","mm","285"]
["Poids","Unité","","","kg","34"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","780"]
["","","Chauffage","Extra lent","tr/min","740"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","10"]
["","","","Max.","°CBS","46"]
["","Chauffage","Temp. ambiante","Min.","°CBH","-15"]
["","","","Max.","°CBH","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46"]
["","Chauffage","","Haut","dBA","47"]
["","","","Bas","dBA","44"]
["Réfrigérant","Type","","","","R-410A"]
["","Charge","","","kg","1.0"]
["","Charge","","","tCO2Eq","2.1"]
["","PRP","","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","15"]
["Accessoires standard","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]