{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-E"]
[]
[]
[]
[]
["","","","","","ATXF20E5V1B","ATXF25E5V1B","ATXF35E5V1B","ATXF42E5V1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.023","0.023","0.029","0.040"]
["","Chauffage","","Nom.","kW","0.023","0.023","0.029","0.040"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","286","286","286","286"]
["","","","Largeur","mm","770","770","770","770"]
["","","","Profondeur","mm","225","225","225","225"]
["Poids","Unité","","","kg","8","8","8.5","9.00"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","9.8","10","11.5","12.6"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8","8","8","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6","6.2","6.4","6.9"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.3","4.3","4.4","4.9"]
["","","Chauffage","Haut","m³/min","10.4","10.4","11.9","12.8"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.3","8.4","8.6","8.8"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.2","6.4","6.5","6.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.3","5.3","5.3","5.2"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","53","54","54","59.0"]
["","Chauffage","","","dBA","55","55","56","59.0"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","39","40","43","45.0"]
["","Refroidissement","","Moyen","dBA","33","33","34","36.0"]
["","","","Bas","dBA","25","26","27","30.0"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","20","20","22.0"]
["","Chauffage","","Haut","dBA","39","40","40","44.0"]
["","","","Moyen","dBA","34","34","35","34.0"]
["","","","Bas","dBA","28","28","29","28.0"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","21","21","22.0"]
["Raccords de tuyauterie","Liquide","","DE","mm","6","6","6","6"]
["","Gaz","","DE","mm","9.5","9.5","9.5","9.50"]
["","Évacuation","","","","18","18","18","18"]
["Systèmes de contrôle","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Systèmes de commande","Télécommande câblée","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50","50","50","50"]
["","Alimentation électrique-=-Tension","","Tension","","220-440","220-440","220-440","220-440"]