{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC073"]
[]
[]
[]
[]
["","","","","BRC073A1"]
["Emballage","Matériau","","","Carton_"]
["","Poids","","kg","0.050"]
["Température extérieure","Humidité relative <","","%","95"]
["","Stockage","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Fonctionnement","Min.","°C","-10"]
["","","Max.","°C","50"]
["Réglage de température","Résolution","","°C","1"]
["","Plage de consigne","Rafraîchissement","°C","18-32"]
["","","Chauffage","°C","10-30"]
["Dimensions","Unité emballée","Largeur","mm","220"]
["","","Hauteur","mm","50"]
["","","Profondeur","mm","160"]
["","Unité","Largeur","mm","120"]
["","","Profondeur","mm","19"]
["","","Hauteur","mm","120"]
["Caisson","Couvercle de boutons","","","non"]
["","Couleur","","","Blanc frais"]
["","DEL de fonctionnement","Couleur","","Vert"]
["Écran LCD","Type","","","\"Full dot\" (160 x 255)"]
["","Rétroéclairage","Couleur","","Blanc"]
["","Dimensions","Largeur","mm","68.85"]
["","","Hauteur","mm","43.2"]
["Poids","Unité emballée","","kg","0.348"]
["","Unité","","kg","0.290"]