{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53A"]
[]
[]
[]
[]
["","","","","BRC1E53A7"]
["Caisson","Couleur","","","Blanc frais"]
["","Couvercle de boutons","","","non"]
["","DEL de fonctionnement","Couleur","","Vert"]
["Dimensions","Unité","Hauteur","mm","120"]
["","","Largeur","mm","120"]
["","","Profondeur","mm","19"]
["","Unité emballée","Hauteur","mm","55"]
["","","Largeur","mm","160"]
["","","Profondeur","mm","150"]
["Poids","Unité","","kg","0.200"]
["","Unité emballée","","kg","0.415"]
["Emballage","Matériau","","","Carton_"]
["","Poids","","kg","0.05"]
["Écran LCD","Type","","","\"Full dot\" (160 x 255)"]
["","Dimensions","Hauteur","mm","43.2"]
["","","Largeur","mm","68.85"]
["","Rétroéclairage","Couleur","","Blanc"]
["Température extérieure","Fonctionnement","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Stockage","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Humidité relative <","","%","95"]
["Raccords de câblage","Longueur de câble","Max.","m","500"]
["Sauvegarde en cas de panne de courant","","","","Oui (Le fonctionnement de l'horloge continue pendant 48 heures maximum.)"]