{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-N"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 3MXM68N2V1B","CHYHBH05AAV32 / 3MXM52N2V1B","CHYHBH05AFV32 / 3MXM52N2V1B","CHYHBH05AFV32 / 3MXM68N2V1B"]
["Production d'eau chaude sanitaire","Général","","Profil de charge déclaré","","XL","XL"]
["","Climat tempéré","","Classe d'efficacité énergétique du chauffage de l'eau","","A","A"]
["COP","","","","","3.91 (1)","4.49 (1)","4.49","3.91"]
["Chauffage des locaux","Sortie d'eau sous climat tempéré : 55 °C","Général","Seasonal space heating eff. class","","A+","A+"]
["","","","ηs (effic. saisonnière du chauffage d'ambiance)","%","113.3","111.4"]
["","","","SCOP","","2.91","2.86"]
["Puissance calorifique","Nom.","","","kW","4.50 (1)","4.41 (1)"]
["Remarques","","","","","(1) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière","(1) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière","(1) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière","(1) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière"]
["Puissance calorifique","Nom.","","","kW","","","4.41","4.5"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","","","XL","XL"]
["","Climat moyen","","Classe","","","","A","A"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-SCOP","","","","2.86","2.91"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","","","A+","A+"]