{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-N9"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 3MXM68N2V1B9"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","XL"]
["","Climat moyen","","Classe d'efficacité énergétique du chauffage de l'eau","","A"]
["COP","","","","","3.91 (1)"]
["Chauffage des locaux","Sortie d'eau sous climat tempéré: 55 °C","Général","Seasonal space heating eff. class","","A+"]
["","","","ηs (effic. saisonnière du chauffage d'ambiance)","%","113.3"]
["","","","SCOP","","2.91"]
["Puissance calorifique","Nom.","","","kW","4.50 (1)"]
["Remarques","","","","","(1) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière"]