{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32","CHYHBH05AFV32","CHYHBH08AFV32"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc"]
["","Matériau","","","","Tôle avec précouche","Tôle avec précouche","Tôle avec précouche"]
["Dimensions","Unité","","Hauteur","mm","902","902","902"]
["","","","Largeur","mm","450","450","450"]
["","","","Profondeur","mm","164","164","164"]
["Poids","Unité","","","kg","30.0","30.0","30.0"]
["DESP","Catégorie","","","","","Art. 3 §3, Hors du champ d'appl. de la dir. rel. aux équip. sous pression (D.E.S.P.) en rais. de l'art. 1, élément 3.6 de la dir. 97/23/CE","Art. 3 §3, Hors du champ d'appl. de la dir. rel. aux équip. sous pression (D.E.S.P.) en rais. de l'art. 1, élément 3.6 de la dir. 97/23/CE"]
["Échangeur de chaleur - côté eau","Débit d'eau","Chauffage","Max.","l/min","23.0 (5)","23.0 (5)","23.0 (5)"]
["Niveau de puissance sonore","Nom.","","","dBA","42 (6)","42 (6)","42 (6)"]
["Plage de fonctionnement","Heating","Côté eau","Min.","°C","25 (7)","25 (7)","25 (7)"]
["Plage de fonctionnement","Chauffage","Côté eau","Max.","°C","50 (7)","50 (7)","50 (7)"]
["Alimentation électrique","Nom","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","230","230","230"]
["Raccords de câblage","Pour raccordement à l'interface utilisateur","","Quantité","","2","2","2"]
["","","","Remarque","","0,75 mm² à 1,25 mm² (longueur max 500 m)","0,75 mm² à 1,25 mm² (longueur max 500 m)","0,75 mm² à 1,25 mm² (longueur max 500 m)"]
["Remarques","","","","","(1) - Pour unité intérieure uniquement","(1) - Pour unité intérieure uniquement","(1) - Pour unité intérieure uniquement"]
["","","","","","(2) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière","(2) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière","(2) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière"]
["","","","","","(3) - 7 °C/6 °C BS/BH - LWC 45 ℃ (DT=5 °C), dérivation de chaudière","(3) - 7 °C/6 °C BS/BH - LWC 45 ℃ (DT=5 °C), dérivation de chaudière","(3) - 7 °C/6 °C BS/BH - LWC 45 ℃ (DT=5 °C), dérivation de chaudière"]
["","","","","","(4) - Min. required","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Dérivation de chaudière","(5) - Dérivation de chaudière","(5) - Dérivation de chaudière"]
["","","","","","(6) - Conformément à la norme EN14825","(6) - Conformément à la norme EN14825","(6) - Conformément à la norme EN14825"]
["","","","","","(7) - Pour connaître la plage de fonctionnement de *HYHB* et *HYKOMB33AA, se reporter au schéma de plage de fonctionnement","(7) - Pour connaître la plage de fonctionnement de *HYHB* et *HYKOMB33AA, se reporter au schéma de plage de fonctionnement","(7) - Pour connaître la plage de fonctionnement de *HYHB* et *HYKOMB33AA, se reporter au schéma de plage de fonctionnement"]