{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BS"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BS"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.02"]
["","Chauffage","","Nom.","kW","0.02"]
["Caisson","Couleur","","","","Argent"]
["Dimensions","Unité","","Hauteur","mm","295"]
["","","","Largeur","mm","798"]
["","","","Profondeur","mm","189"]
["Poids","Unité","","","kg","11.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","11"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6.1"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.6"]
["","","Chauffage","Haut","m³/min","10.9"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.7"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","57"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","39"]
["","Refroidissement","","Moyen","dBA","32"]
["","","","Bas","dBA","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["","Chauffage","","Haut","dBA","39"]
["","","","Moyen","dBA","32"]
["","","","Bas","dBA","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["Réfrigérant","PRP","","","","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.5"]
["","Évacuation","","","","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A58"]
["","Télécommande câblée","","","","BRC073"]
["Accessoires standard","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Filtre à air","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Alimentation électrique","Nom","","","","V1"]
["","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]