{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.02"]
["","Chauffage","","Nom.","kW","0.02"]
["Caisson","Couleur","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","600"]
["","","","Largeur","mm","750"]
["","","","Profondeur","mm","238"]
["Poids","Unité","","","kg","17"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","8.7"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","4.9"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1"]
["","","Chauffage","Haut","m³/min","9.2"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","7.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","5.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","52"]
["","Chauffage","","","dBA","52"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","38"]
["","Refroidissement","","Moyen","dBA","32"]
["","","","Bas","dBA","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","22"]
["","Chauffage","","Haut","dBA","38"]
["","","","Moyen","dBA","32"]
["","","","Bas","dBA","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["Réfrigérant","PRP","","","","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.4"]
["","Gaz","","DE","mm","9.5"]
["","Évacuation","","","","VP20 (I.D. 20/O.D. 26)"]
["Systèmes de contrôle","Infrared remote control","","","","ARC466A66"]
["Systèmes de commande","Télécommande câblée","","","","BRC073A1"]
["Accessoires standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]