{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A1A"]
[]
[]
[]
[]
["","","","","","D2CND024A1AA","D2CND024A1AB","D2CND028A1AA","D2CND028A1AB","D2CND035A1AA","D2CND035A1AB"]
["Gaz","Consommation (G20)","","Min.","m³/h","0.31","0.31","0.511","0.511","0.511","0.511"]
["","","","Max.","m³/h","2.48","2.48","2.89","2.89","3.63","3.63"]
["","Consommation (G25)","","Min.","m³/h","0.36","0.36","0.59","0.59","0.59","0.59"]
["","","","Max.","m³/h","2.89","2.89","3.32","3.32","4.19","4.19"]
["","Consommation (G31)","","Min.","m³/h","0.12","0.12","0.2","0.2","0.2","0.2"]
["","","","Max.","m³/h","0.96","0.96","1.1","1.1","1.38","1.38"]
["","Catégorie NOx","","","","6","6","6","6","6","6"]
["","Niveau NOx (G20)","","","mg/kWh","22","22","36.3","36.3","35.5","35.5"]
["Chauffage central","Apport de chaleur Qn (valeur calorifique nette)","Nom.","Min.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max.","kW","23.5","23.5","27","27","34","34"]
["","Apport de chaleur Qn (valeur calorifique brute)","Nom.","Min.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max.","kW","26.1","26.1","30","30","37.8","37.8"]
["","Chauffage central-=-Sortie Pn à 80/60&nbsp;°C","","Chauffage central-=-Sortie Pn à 80/60&nbsp;°C-=-Min.-=-kW","kW","2.8","2.8","4.6","4.6","4.6","4.6"]
["","","","Chauffage central-=-Sortie Pn à 80/60&nbsp;°C-=-Nom.-=-kW","kW","22.8","22.8","26.3","26.3","33.2","33.2"]
["","Chauffage central-=-Sortie Pnc à 50/30&nbsp;°C","","Chauffage central-=-Sortie Pnc à 50/30&nbsp;°C-=-Min.-=-kW","kW","3.1","3.1","5.2","5.2","5.2","5.2"]
["","","","Chauffage central-=-Sortie Pnc à 50/30&nbsp;°C-=-Nom.-=-kW","kW","24.0","24","28.2","28.2","35","35"]
["","Chauffage central-=-Sortie à 37/30&nbsp;°C","","Chauffage central-=-Sortie à 37/30&nbsp;°C-=-Nom.-=-kW","kW","7.6","7.6","8.8","8.8","11.1","11.1"]
["","Température de l'eau","","Max.","°C","100","100","100","100","100","100"]
["","Efficacité","","Valeur calorique nette","%","97.9","97.9"]
["","","","Valeur calorique brute","%","87.3","87.3"]
["Eau chaude sanitaire","Apport de chaleur (valeur calorifique nette) Qnw","Nom.","Min.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max.","kW","23.5","23.5","29.5","29.5","34","34"]
["","Apport de chaleur (valeur calorifique brute) Qnw","Nom.","Min.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max.","kW","26.1","26.1","32.7","32.7","37.7","37.7"]
["","Température","","Max.","°C","60","60","60","60","60","60"]
["Pertes thermiques","Chaudière de réserve Ps","","","kW","0.057","0.057","0.0650","0.065","0.0650","0.065"]
["Air d'alimentation","Connexion","","","mm","100","100","100","100","100","100"]
["","Concentrique","","","","Oui","Oui","Oui","Oui","Oui","Oui"]
["Gaz de carneau","Température","","Max.","°C","90","90","76.4","76.4","81.7","81.7"]
["","Connexion","","","mm","60","60","60","60","60","60"]
["","Débit massique (G20)","","Max.","kg/h","38.7","38.7","44.5","55.7","55.7","55.7"]
["","Débit massique (G25)","","Max.","kg/h","","","39.3","39.3","49.6","49.6"]
["","Débit massique (G31)","","Max.","kg/h","36.0","36","43.3","43.3","54.7","54.7"]
["Caisson","Couleur","","","","Blanc titane (Ral9003)","Blanc titane (Ral9003)","Blanc titane (Ral9003)","Blanc titane (Ral9003)","Blanc titane (Ral9003)","Blanc titane (Ral9003)"]
["","Matériau","","","","Tôle","Tôle","Tôle d'acier galvanisée, revêtue d'une couche de peinture en poudre","Tôle d'acier galvanisée, revêtue d'une couche de peinture en poudre","Tôle d'acier galvanisée, revêtue d'une couche de peinture en poudre","Tôle d'acier galvanisée, revêtue d'une couche de peinture en poudre"]
["Dimensions","Unité","Hauteur","Caisson","mm","590","590","690","690","690","690"]
["","","","Largeur","mm","400","400","440","440","440","440"]
["","","","Profondeur","mm","256","256","295","295","295","295"]
["Poids","Unité","","Vide","kg","27","27","37","37","37","37"]
["","","","Pleine","kg","27","27","39","","39"]
["","Chaudière","","Vide","kg","27.0","27"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","XL","XL","XL","XL","XL","XL"]
["Production d'eau chaude sanitaire","Général","","Classe","","A","A","A","A","A","A"]
["Chauffage de l'air ambiant","Général","","Classe d'efficacité saisonnière du chauffage de l'air ambiant","","A","A","A","A","A","A"]