{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Température extérieure","Humidité relative <","","","%","85"]
["Nombre maximum d'unités intérieures connectables","","","","","32"]
["Puissance absorbée","kW","","","","0.015 (1)"]
["Communication","DIII-NET","","Quantité","","1"]
["","","","Remarque","","DIII-NET (F1F2)"]
["","Ethernet","","Quantité","","1"]
["","Borne d’entrée","Numérique","Quantité","","4"]
["Dimensions","Unité","","Largeur","mm","384"]
["","","","Profondeur","mm","92"]
["","","","Hauteur","mm","136"]
["Nombre maximum d'unités extérieures connectables","","","","","7"]
["Power supply","Fréquence","","","Hz","50/60"]
["","Tension","","","V","110-240 (alimentation externe)"]
["Remarques","","","","","(1) - Inclut la puissance absorbée de l'alimentation WAGO, le module UC et le module E/S"]
["","","","","","(2) - Les dimensions incluent l'alimentation WAGO, le module UC, le module E/S et l'espace nécessaire entre les différents éléments."]
["","","","","","(3) - Dimensions de l'écran optionnel : hauteur : 209 mm, largeur : 123 mm, profondeur : 8,5 mm"]