{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM010A51"]
[]
[]
[]
[]
["","","","","DCM010A51."]
["Unité connectable","","","","Types intérieur, extérieur, hydrobox, ventilation de points de gestion iTM"]
["Entrée","PC","Logiciel","","Microsoft Windows 7, 8, 8.1, 10, Microsoft Server 2012 et 2016"]
["Nombre maximum d'unités intérieures connectables","","","","2,500 (2)"]
["Nombre maximum d'unités extérieures connectables","","","","400 (3)"]
["Remarques","","","","(1) - Versions Oracle PMS compatibles : Opera v5.0.03.03 e43, v5.0.04.01 e24, v5.0.04.02 e17, v5.0.04.02 e17, v5.0.04.03 e10, v5.0.05.00 et ultérieures"]
["","","","","(2) - 5 x 500 unités intérieures par dispositif de commande iTM"]
["","","","","(3) - Température intérieure : 29 °CBS, 19 °CBH ; température extérieure : 46 ° CBS, 24 ° CBH"]
["","","","","(4) - Température intérieure : 29 °CBS, 19 °CBH ; température extérieure : 46 ° CBS, 24 ° CBH"]
["","","","","(5) - Température intérieure : 29 °CBS, 19 °CBH ; température extérieure : 46 ° CBS, 24 ° CBH"]