{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D"]
[]
[]
[]
[]
["","","","","","EBSXB11P30DF","EBSXB11P50DF","EBSXB11P30DG","EBSXB11P50DG","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DG","EBSXB16P50DG"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)"]
["","Matériau","","","","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc"]
["Dimensions","Unité","","Hauteur","mm","1,893","1,910","1,893","1,910","1,893","1,910","1,893","1,910"]
["","","","Largeur","mm","594","792","594","792","594","792","594","792"]
["","","","Profondeur","mm","680","817","680","817","680","817","680","817"]
["Poids","Unité","","","kg","94","117","94","117","94","117","94","117"]
["DESP","Catégorie","","","","Catégorie II","Catégorie II","Catégorie II","Catégorie II","Catégorie II","Catégorie II","Catégorie II","Catégorie II"]
["Réfrigérant","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","PRP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Charge","","","kg","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Niveau de puissance sonore","Nom.","","","dBA","44.7","44.7","44.7","44.7","49.0","49.0","49.0","49.0"]
["Niveau de pression sonore","Nom.","","","dBA","36.8","36.8","36.8","36.8","40.3","40.3","40.3","40.3"]
["Plage de fonctionnement","Chauffage","Côté eau","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Rafraîchissement","Temp. ambiante","Min.","°CBS","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Côté eau","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50","50","50"]
["","Tension","","","V","230","230","230","230","230","230","230","230"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(2) - Se reporter au schéma de limites de fonctionnement","(2) - Se reporter au schéma de limites de fonctionnement","(2) - Se reporter au schéma de limites de fonctionnement","(2) - Se reporter au schéma de limites de fonctionnement","(2) - Se reporter au schéma de limites de fonctionnement","(2) - Se reporter au schéma de limites de fonctionnement","(2) - Se reporter au schéma de limites de fonctionnement","(2) - Se reporter au schéma de limites de fonctionnement"]