{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Niveau de pression sonore","Nom.","","","dBA","32.0 (6)"]
["Réfrigérant","PRP","","","","2,090"]
["","Charge","","","kg","1.80"]
["","Type","","","","R-410A"]
["Plage de fonctionnement","Espace d'installation","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Heating","Côté eau","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Côté saumure","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Eau chaude domestique","Côté eau","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Puissance absorbée","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Niveau de puissance sonore","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Dimensions","Unité","","Largeur","mm","600"]
["","","","Profondeur","mm","728"]
["","","","Hauteur","mm","1,730"]
["Caisson","Matériau","","","","Tôle avec précouche"]
["","Colour","","","","Blanc"]
["Ballon","Protection contre la corrosion","","","","Anode"]
["","Isolation","","Perte thermique","kWh/24 h","1.36 (4)"]
["Poids","Unité","","","kg","210"]
["Chauffage des locaux","Sortie d'eau climat tempéré 35 °C","Général","ηs (effic. saisonnière du chauffage d'ambiance)","%","194"]
["","","","Classe d'effic. saisonnière du chauffage d'ambiance","","A+++"]
["","","","SCOP","","5.06"]
["","Sortie d'eau sous climat tempéré 55 °C","Général","Seasonal space heating eff. class","","A++"]
["","","","ηs (effic. saisonnière du chauffage d'ambiance)","%","139"]
["","","","SCOP","","3.68"]
["Puissance calorifique","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Phase","","","","3~"]
["","Nom","","","","9W"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","400"]
["Courant","Fusibles recommandés","","","A","25"]
["Remarques","","","","","(1) - EWB/LWB 0 °C/-3 °C - LWC 35 °C (DT=5 °C)"]
["","","","","","(2) - EWB/LWB 0 °C/-3 °C - LWC 45 °C (DT=5 °C)"]
["","","","","","(3) - avec 40 % de propylène glycol"]
["","","","","","(4) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(5) - Tuyauterie + échangeur de chaleur à plaques (PHE) + chauffage de secours inclus ; vase d'expansion exclus"]
["","","","","","(6) - Le niveau de pression sonore est mesuré à l'aide d'un microphone placé à 1 m de l'unité. Il s'agit d'une valeur relative qui varie en fonction de la distance et de l'environnement acoustique."]
["","","","","","(7) - Par pompe à chaleur"]
["","","","","","(8) - Par pompe à chaleur + dispositif de chauffage de secours"]
["","","","","","(9) - Par dispositif de chauffage de secours"]