{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSXB07A"]
[]
[]
[]
[]
["","","","","","EPSXB07P30AF","EPSXB07P50AF"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016), Noir graphite (RAL9011), Noir jet (RAL9005)","Blanc signalisation (RAL9016), Noir graphite (RAL9011), Noir jet (RAL9005)"]
["","Matériau","","","","Polypropylène anti-choc","Polypropylène anti-choc"]
["Dimensions","Unité","","Hauteur","mm","1914","1906"]
["","","","Largeur","mm","590","785"]
["","","","Profondeur","mm","671","837"]
["Poids","Unité","","","kg","87.0","109"]
["DESP","Catégorie","","","","Art 4.3","Art 4.3"]
["Niveau de puissance sonore","Nom.","","","dBA","47.0","47.0"]
["Niveau de pression sonore","Nom.","","","dBA","24.8","24.8"]
["Plage de fonctionnement","Chauffage","Côté eau","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["","Rafraîchissement","Temp. ambiante","Min.","°CBS","0 (3)","0 (3)"]
["","","Côté eau","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","230","230"]
["Dispositif de chauffage électrique","Alimentation électrique","","Nom","","6V / 9W","6V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~"]
["","","","Fréquence","Hz","50","50"]
["","","","Tension","V","230/400","230/400"]
["","Fusibles recommandés","","","A","0.000 (4)","0.000 (4)"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(2) - Volume minimum requis, volume dans l'unité exclus","(2) - Volume minimum requis, volume dans l'unité exclus"]
["","","","","","(3) - Se reporter au schéma de limites de fonctionnement","(3) - Se reporter au schéma de limites de fonctionnement"]
["","","","","","(4) - Se reporter au schéma de câblage et au manuel d'installation pour le fusible recommandé en fonction de l’alimentation et du raccordement au réseau","(4) - Se reporter au schéma de câblage et au manuel d'installation pour le fusible recommandé en fonction de l’alimentation et du raccordement au réseau"]