{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB16E"]
[]
[]
[]
[]
["","","","","","ETSXB16P50EF","ETSXB16P30EF"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)"]
["","Matériau","","","","Polypropylène anti-choc","Polypropylène anti-choc"]
["Dimensions","Unité","","Hauteur","mm","1,910","1,892"]
["","","","Largeur","mm","792","594"]
["","","","Profondeur","mm","816","644"]
["Poids","Unité","","","kg","100","76"]
["Sound power level","Nom.","","","dBA","45.6","45.6"]
["Niveau de pression sonore","Nom.","","","dBA","32.8","32.8"]
["Plage de fonctionnement","Chauffage","Côté eau","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["","Rafraîch.","Temp. ambiante","Min.","°CBS","0 (2)","0 (2)"]
["","","Côté eau","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["Power supply","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","230","230"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(2) - Se reporter aux schémas de limites de fonctionnement","(2) - Se reporter aux schémas de limites de fonctionnement"]