{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["","Matériau","","","","Résine","Résine"]
["Dimensions","Unité","","Hauteur","mm","290","340"]
["","","","Largeur","mm","1050","1200"]
["","","","Profondeur","mm","269","262"]
["Poids","Unité","","","kg","14","18"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","16.2","23"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","13.4","21.1"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","12.1","18.7"]
["","","Chauffage","Haut","m³/min","16.9","23"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","14.2","20.9"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","12.7","18.7"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","61","65"]
["","Chauffage","","","dBA","61","65"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","45","49"]
["","Refroidissement","","Moyen","dBA","42","45"]
["","","","Bas","dBA","40","41"]
["","Chauffage","","Haut","dBA","45","49"]
["","","","Moyen","dBA","42","45"]
["","","","Bas","dBA","40","41"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","9.52"]
["","Gaz","","DE","mm","15.9","15.9"]
["","Évacuation","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","220-240","220-240"]
["Accessoires standard","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Remarques","","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["Accessoires standard","Screw cover","","","","","3"]