{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":12,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9)"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB9","FBA50A2VEB9","FBA60A2VEB9","FBA71A2VEB9","FBA100A2VEB","FBA125A2VEB","FBA140A2VEB"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","","","","","","14.00","15.40"]
["Puissance calorifique","Puissance totale","","Nom.","kW","","","","","","13.5","15.5"]
["Caisson","Couleur","","","","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)"]
["","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","245","245","245","245","245","245","245"]
["","","","Largeur","mm","700","700","1000","1000","1400","1400","1400"]
["","","","Profondeur","mm","800","800","800","800","800","800","800"]
["Poids","Unité","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","","Chauffage","Haut","m³/min","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","Pression statique externe","","Nom.","Pa","30","30","30","30","40","50","50"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60.0","60.0","56.0","56.0","58.0","62.0","62.0"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","35.0","35.0","30.0","30.0","34.0","37.0","37.0"]
["","Refroidissement","","Moyen","dBA","32.0","32.0","28.0","28.0","32.0","35.0","35.0"]
["","","","Bas","dBA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["","Chauffage","","Haut","dBA","37.0","37.0","31.0","31.0","36.0","38.0","38.0"]
["","","","Moyen","dBA","34.0","34.0","28.0","28.0","33.0","35.0","35.0"]
["","","","Bas","dBA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaz","","DE","mm","9.52","12.70","12.70","15.90","15.90","15.90","15.90"]
["","Évacuation","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Hauteur manométrique","mm","","","","625","625","625","625","625","625","625"]
["Systèmes de commande","Télécommande infrarouge","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Télécommande câblée","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accessoires standard","Installation manual","","","","1","1","1","","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","","8","8","8"]
["","Operation manual","","","","1","1","1","","1","1","1"]
["","Clamps","","","","4","4","4","","4","4","4"]
["","Drain hose","","","","1","1","1","","1","1","1"]
["","Insulation for fitting","","","","2","2","2","","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","","1","1","1"]
["","Screws","","","","40","40","40","","40","40","40"]
["","Sealing pads","","","","5","5","5","","5","5","5"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Tension","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Accessoires standard","Manuel d'installation","","","","","","","1"]
["","Rondelle pour attache de suspension","","","","","","","8"]
["","Manuel d’utilisation","","","","","","","1"]
["","Attaches","","","","","","","4"]
["","Flexible d'évacuation","","","","","","","1"]
["","Isolant pour raccord","","","","","","","2"]
["","Bride métallique pour flexible d'évacuation","","","","","","","1"]
["","Vis","","","","","","","40"]
["","Tampons d’étanchéité","","","","","","","5"]
["Remarques","","","","","","","","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]
["","","","","","","","","(2) - Pour les données électriques, se reporter au schéma séparé.","","(2) - Pour les données électriques, se reporter au schéma séparé."]