{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D"]
[]
[]
[]
[]
["","","","","","FBQ35D2VEB","FBQ50D2VEB","FBQ60D2VEB","FBQ71D2VEB","FBQ100D2VEB","FBQ125D2VEB","FBQ140D2VEB"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","37","37","31","31.0","36.0","38.0","38"]
["","","","Moyen","dBA","34","34","28","28.0","33.0","35.0","35"]
["","","","Bas","dBA","29","29","25","25.0","30.0","32.0","32"]
["","Rafraîchissement","","Moyen","dBA","32","32","28","28.0","32.0","35.0","35"]
["","","","Bas","dBA","29","29","25","25.0","30.0","32.0","32"]
["","","","Haut","dBA","35","35","30","30.0","34.0","37.0","37"]
["Accessoires standard","Manuel d’utilisation","","","","1","1","1","1","1","1","1"]
["","Manuel d'installation","","","","1","1","1","1","1","1","1"]
["","Flexible d'évacuation","","","","1","1","1","1","1","1","1"]
["","Bride métallique pour flexible d'évacuation","","","","1","1","1","1","1","1","1"]
["","Rondelle pour attache de suspension","","","","8","8","8","8","8","8","8"]
["","Vis","","","","40","40","40","40","40","40","40"]
["","Isolant pour raccord","","","","2","2","2","2","2","2","2"]
["","Tampon d’étanchéité","","","","5","5","5","5","5","5","5"]
["","Tampons d’étanchéité","","","","","","","5","5","5","5"]
["","Attaches","","","","4","4","4","4","4","4","4"]
["Réfrigérant","PRP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Systèmes de commande","Télécommande câblée","","","","","","","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528"]
["","Infrared remote control","","","","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Raccordements de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaz","","DE","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Evacuation","","","","VP20 (D.I. 20/D.E. 26), hauteur de refoulement 625 mm","VP20 (D.I. 20/D.E. 26), hauteur de refoulement 625 mm","VP20 (D.I. 20/D.E. 26), hauteur de refoulement 625 mm","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Rafraîchissement","","","dBA","60","60","56","56","58","62","62"]
["Dimensions","Unité","","Largeur","mm","700","700","1,000","1,000","1,400","1,400","1,400"]
["","","","Profondeur","mm","800","800","800","800","800","800","800"]
["","","","Hauteur","mm","245","245","245","245","245","245","245"]
["Caisson","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["","Couleur","","","","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)"]
["Poids","Unité","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ventilateur","Pression statique externe","","Haute","Pa","150","150","150","150","150","150","150"]
["","","","Nom.","Pa","30","30","30","30","40","50","50"]
["","Débit d'air","Chauffage","Haut","m³/min","","","","","29.0","34.0","34.0"]
["","","","Bas","m³/min","","","","","23.0","23.5","23.5"]
["","","","Moyen","m³/min","","","","","26.0","29.0","29.0"]
["","","Rafraîchissement","Bas","m³/min","","","","","23.0","23.5","23.5"]
["","","","Moyen","m³/min","","","","","26.0","29.0","29.0"]
["","","","Haut","m³/min","","","","","29.0","34.0","34.0"]
["Hauteur manométrique","mm","","","","625","625","625","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Nom","","","","VE","VE","VE","VE","VE","VE","VE"]
["","Tension","","","V","220-240","220-240","220-240","220-240/220","220-240/220","220-240/220","220-240/220"]
["Remarques","","","","","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]