{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG100AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG140AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B","FCAG140AVEB / RZQG140L7Y1B"]
["Puissance frigorifique","Nom.","","kW","","","","","","","","","","6.80 (1)","","","","","","13.4 (1)","13.4 (1)"]
["Rafraîchissement de l'air ambiant","SEER","","","","","","","","","","5.10","5.10","6.72","","","","","","9.70","6.44"]
["","ηs,c","","%","","","","","","","","","","","","","","","","385.1","254.6"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","","467","467","355","","","","","","829","1,249"]
["","Puissance","Pdesign","kW","","","","","","","","6.80","6.80","6.80","","","","","","13.4","13.4"]
["","Classe d’efficacité énergétique","","","","","","","","","","A","A","A++"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","","","","","","","","6.00","6.00","6.33","","","","","","12.0","11.6"]
["","SCOP/A","","","","","","","","","","3.80","3.80","4.20","","","","","","3.96","4.27"]
["","Classe d’efficacité énergétique","","","","","","","","","","A","A","A+"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","","2,211","2,211","2,110","","","","","","4,235","3,795"]
["","ηs,h","","%","","","","","","","","","","","","","","","","155.2","167.6"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","","","","","","","","","1,005"]
["","EER","","","","","","","","","","","","3.39 (3)","","","","","","4.29 (3)","2.50 (3)"]
["","COP","","","","","","","","","","","","3.97 (3)","","","","","","","3.61 (3)"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","","","","","","","","","A"]
["","","Chauffage","","","","","","","","","","","A"]
["Puissance calorifique","Nom.","","kW","","","","","","","","","","7.50 (2)","","","","","","15.5 (2)","15.5 (2)"]
["Remarques","","","","","","","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m","","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","","","","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m","","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]
["","","","","","","","","","","","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","","","","","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["Classe d'efficacité énergétique","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Unité extérieure","","","","","","","","","","","","","","RZQG71L8Y1","RZQG100L8Y1","RZQG100L8Y1","RZQG125L8Y1","RZQG125L8Y1"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","","","","","","","","","","","A++","A","A++","A","A+"]
["","Puissance","Pdesign","kW","","","","","","","","","","","6.80","9.50","9.50","12.0","12.00"]
["","SEER","","","","","","","","","","","","","6.72","5.10","6.80","5.10","6.00"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","","","","","355","652","489","824","700"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","","","","","","","","","","A+","A","A++","A","A+"]
["","Puissance","Pdesign","kW","","","","","","","","","","","6.33","11.3","11.30","12.7","12.66"]
["","SCOP/A","","","","","","","","","","","","","4.20","3.80","4.61","3.80","4.10"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","","","","","2110","4164","3432","4683","4323"]