{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":12,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B"]
[]
[]
[]
[]
["","","","","","FCAG35BVEB","FCAG50BVEB","FCAG60BVEB","FCAG71BVEB","FCAG100BVEB","FCAG125BVEB","FCAG140BVEB"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","3.50","5.00","5.70","6.80","9.50","12.10","13.40"]
["Puissance calorifique","Puissance totale","","Nom.","kW","4.2","6.0","7.0","7.5","10.8","13.5","15.5"]
["Caisson","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","204","204","204","204","246","246","246"]
["","","","Largeur","mm","840","840","840","840","840","840","840"]
["","","","Profondeur","mm","840","840","840","840","840","840","840"]
["Poids","Unité","","","kg","18","19","19","21","23","23","23"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","12.9","14.6","14.9","15.1","22.7","27.2","27.2"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","10.6","11.8","12.2","13","17.8","20.4","20.4"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","8.8","9.4","9.6","10.8","13","13.1","13.1"]
["","","Chauffage","Haut","m³/min","14.1","14.6","14.9","15.1","23","27","27"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","11.6","11.8","12.2","12.9","18.1","20.2","20.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","9.4","9.4","9.6","10.8","13.2","13","13"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","49","49","51","51","54","58","58"]
["","Chauffage","","","dBA","49","49","51","51","54","58","58"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","31","31","33","35","37","41","41"]
["","Refroidissement","","Moyen","dBA","29","29","31","31","33","35","35"]
["","","","Bas","dBA","27","27","28","28","29","29","29"]
["","Chauffage","","Haut","dBA","31","31","33","33","37","41","41"]
["","","","Moyen","dBA","29","29","31","31","33","35","35"]
["","","","Bas","dBA","27","27","28","28","29","29","29"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaz","","DE","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Évacuation","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Panneau décoratif","Modèle","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Dimensions","","Hauteur","mm","65","65","65","65","65","65","65"]
["","","","Largeur","mm","950","950","950","950","950","950","950"]
["","","","Profondeur","mm","950","950","950","950","950","950","950"]
["","Poids","","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["Panneau décoratif 2","Panneau décoratif 2-=-Modèle","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Panneau décoratif 2-=-Dimensions","","Panneau décoratif 2-=-Dimensions-=-Hauteur-=-mm","mm","148","148","148","148","148","148","148"]
["","","","Panneau décoratif 2-=-Dimensions-=-Largeur-=-mm","mm","950","950","950","950","950","950","950"]
["","","","Panneau décoratif 2-=-Dimensions-=-Profondeur-=-mm","mm","950","950","950","950","950","950","950"]
["","Panneau décoratif 2-=-Poids-=-kg","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["Panneau décoratif 3","Panneau décoratif 3-=-Modèle","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Panneau décoratif 3-=-Dimensions","","Panneau décoratif 3-=-Dimensions-=-Hauteur-=-mm","mm","106","106","106","106","106","106","106"]
["","","","Panneau décoratif 3-=-Dimensions-=-Largeur-=-mm","mm","950","950","950","950","950","950","950"]
["","","","Panneau décoratif 3-=-Dimensions-=-Profondeur-=-mm","mm","950","950","950","950","950","950","950"]
["","Panneau décoratif 3-=-Poids-=-kg","","","kg","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["Systèmes de commande","Télécommande infrarouge","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["","Télécommande câblée","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1H81W/S, BRC1H51(9)W/S/K7, BRC2E52C7, BRC3E52C7"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Tension","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]