{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H"]
[]
[]
[]
[]
["","","","","","FCAHG71HVEB","FCAHG100HVEB","FCAHG125HVEB","FCAHG140HVEB"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","6.80","9.50","12.10","13.40"]
["Puissance calorifique","Puissance totale","","Nom.","kW","7.50","10.8","13.5","15.5"]
["Caisson","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","288","288","288","288"]
["","","","Largeur","mm","840","840","840","840"]
["","","","Profondeur","mm","840","840","840","840"]
["Poids","Unité","","","kg","25","25","25","25"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","23.6","32.2","34.4","34.4"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","18.8","25.7","27.3","27.3"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","13.7","19.1","21.2","21.2"]
["","","Chauffage","Haut","m³/min","23.6","30.8","32.1","32.1"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","18.8","24.6","25.5","25.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","13.7","18.3","19.7","19.7"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","53","61","61","61"]
["","Chauffage","","","dBA","53","61","61","61"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","36","44","45","45"]
["","Refroidissement","","Moyen","dBA","33","39","40","41"]
["","","","Bas","dBA","29","33","35","37"]
["","Chauffage","","Haut","dBA","36","44","45","45"]
["","","","Moyen","dBA","33","39","40","41"]
["","","","Bas","dBA","29","33","35","37"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","9.52","9.52","9.52"]
["","Gaz","","DE","mm","15.9","15.9","15.9","15.9"]
["","Évacuation","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Panneau décoratif","Modèle","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Dimensions","","Hauteur","mm","65","65","65","65"]
["","","","Largeur","mm","950","950","950","950"]
["","","","Profondeur","mm","950","950","950","950"]
["","Poids","","","kg","5.5","5.5","5.5","5.5"]
["Panneau décoratif&nbsp;2","Panneau décoratif&nbsp;2-=-Modèle","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Panneau décoratif&nbsp;2-=-Dimensions","","Panneau décoratif&nbsp;2-=-Dimensions-=-Hauteur-=-mm","mm","148","148","148","148"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Largeur-=-mm","mm","950","950","950","950"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Profondeur-=-mm","mm","950","950","950","950"]
["","Panneau décoratif&nbsp;2-=-Poids-=-kg","","","kg","10.3","10.3","10.3","10.3"]
["Panneau décoratif&nbsp;3","Panneau décoratif&nbsp;3-=-Modèle","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Panneau décoratif&nbsp;3-=-Dimensions","","Panneau décoratif&nbsp;3-=-Dimensions-=-Hauteur-=-mm","mm","106","106","106","106"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Largeur-=-mm","mm","950","950","950","950"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Profondeur-=-mm","mm","950","950","950","950"]
["","Panneau décoratif&nbsp;3-=-Poids-=-kg","","","kg","6.5","6.5","6.5","6.5"]
["Systèmes de commande","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["Systèmes de commande","Télécommande câblée","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accessoires standard","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1"]
["","Clamps","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation guide","","","","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2"]
["","Screws","","","","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50/60","50/60","50/60","50/60"]
["","Alimentation électrique-=-Tension","","Tension","","220-240/220","220-240/220","220-240/220","220-240/220"]