{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQG71L7V1B","FCQG35FVEB / FCQG35FVEB / RZQG71L7Y1B9","FCQG71FVEB / RZQG71L7V1B","FCQG100FVEB / RZQG100L7Y1B","FCQG100FVEB / RZQG100L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L7Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L7Y1B"]
["Puissance frigorifique","Nom.","","kW","","","6.8","9.5","9.5"]
["Rafraîchissement de l'air ambiant","SEER","","","4.30","4.30","5.81","5.99","5.99","4.30","4.30","4.30","4.30"]
["","Consommation d’énergie annuelle","","kWh/a","554","554","409.639","555.092","555.092","773.256","773.256","976.744","976.744"]
["","Puissance","Pdesign","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50","12.00","12.00"]
["","Classe d’efficacité énergétique","","","C","C","A+","A+","A+","C","C","C","C"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","6.00","6.00","6.33","11.30","11.30","10.20","10.20","12.71","12.71"]
["","SCOP/A","","","3.40","3.40","4.13","3.93","3.93","3.80","3.80","3.40","3.40"]
["","Classe d’efficacité énergétique","","","A","A","A+","A","A","A","A","A","A"]
["","Consommation d’énergie annuelle","","kWh/a","2,472","2,472","2,145.763","4,027","4,027","3,757","3,757","5,232","5,232"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","","1,005","1,225","1,225"]
["","EER","","","","","3.39","3.87","3.87"]
["","COP","","","","","3.97","4.15","4.15"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","","A","A","A"]
["","","Chauffage","","","","A","A","A"]
["Puissance calorifique","Nom.","","kW","","","7.5","10.8","10.8"]
["Remarques","","","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]
["","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]