{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZAG125M7V1B"]
["Puissance frigorifique","Nom.","","kW","12.1 (1)"]
["Rafraîchissement des locaux","SEER","","","6.59"]
["","Consommation d’énergie annuelle","","kWh/a","1,102"]
["","Puissance","Pdesign","kW","12.1"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","9.52"]
["","SCOP/A","","","4.08"]
["","Consommation d’énergie annuelle","","kWh/a","3,267"]
["Puissance calorifique","Nom.","","kW","13.5 (2)"]
["Remarques","","","","(1) - Les puissances frigorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(4) - Pour les données électriques, se reporter au schéma séparé."]