{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Puissance frigorifique","Nom.","","kW","12.5 (3)"]
["Raccords de tuyauterie","Liquide","DE","mm","9.52"]
["","Gaz","DE","mm","15.9"]
["","Evacuation","DE","mm","26"]
["Rafraîchissement des locaux","SEER","","","3.50"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","B"]
["","","Chauffage","","A"]
["Puissance calorifique","Nom.","","kW","14.0 (4)"]
["Remarques","","","","(1) - Étiquette énergétique : échelle de A (efficacité maximum) à G (efficacité minimum)."]
["","","","","(2) - Consommation énergétique annuelle : basée sur un fonctionnement moyen de 500 heures par an à pleine charge (conditions nominales)"]
["","","","","(3) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 5m ; dénivelé : 0m"]
["","","","","(4) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m ; dénivelé : 0m"]
["","","","","(5) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]