{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B"]
[]
[]
[]
[]
["","","","","","FDQ125B8V3B9","FDQ200B8V3B9","FDQ250B8V3B9"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","","20.0","24.1"]
["Puissance calorifique","Puissance totale","","Nom.","kW","","23.0","26.4"]
["Caisson","Couleur","","","","Non peint","Non peint","Non peint"]
["","Matériau","","","","Acier galvanisé","Acier galvanisé","Acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","350","450","450"]
["","","","Largeur","mm","1,400","1,400","1,400"]
["","","","Profondeur","mm","662","900","900"]
["Poids","Unité","","","kg","59.0","89.0","94.0"]
["Vide de faux-plafond requis >","mm","","","","350","450","450"]
["Ventilateur","Débit d'air","Rafraîchissement","Nom.","m³/min","43.0"]
["","","","Moyen","m³/min","","69.0","89.0"]
["","","Chauffage","Nom.","m³/min","43.0"]
["","","","Moyen","m³/min","","69.0","89.0"]
["","Pression statique externe","","Haute","Pa","150","250","250"]
["","","","Nom.","Pa","150","250","250"]
["","","","Basse","Pa","150","250","250"]
["Sound power level","Rafraîchissement","","","dBA","75.0","81.0","82.0"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","44.0","45.0","47.0"]
["","Chauffage","","Bas","dBA","44.0","45.0","47.0"]
["Raccordements de tuyauterie","Liquide","","DE","mm","9.52","9.52","12.70"]
["","Gaz","","DE","mm","15.9","22.2","22.2"]
["","Evacuation","","","","","OD Ø25.0","OD Ø25.0"]
["Systèmes de commande","Télécommande câblée","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Accessoires standard","Manuel d'installation et d'exploitation","","","","1","1","1"]
["Power supply","Nom","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","230","230 +/-10%","230 +/-10%"]
["Remarques","","","","","(1) - Les valeurs sonores sont mesurées dans une pièce semi-anéchoïque avec des corrections.","(1) - Les valeurs sonores sont mesurées dans une pièce semi-anéchoïque avec des corrections.","(1) - Les valeurs sonores sont mesurées dans une pièce semi-anéchoïque avec des corrections."]
["","","","","","(2) - Le niveau de pression sonore est mesuré à l'aide d'un microphone placé à 1 m de l'unité.","(2) - Le niveau de pression sonore est mesuré à l'aide d'un microphone placé à 1 m de l'unité.","(2) - Le niveau de pression sonore est mesuré à l'aide d'un microphone placé à 1 m de l'unité."]
["","","","","","(3) - Il s'agit d'une valeur relative qui varie en fonction de la distance et de l'environnement acoustique. Pour plus de détails, se reporter aux schémas de niveau sonore.","(3) - Il s'agit d'une valeur relative qui varie en fonction de la distance et de l'environnement acoustique. Pour plus de détails, se reporter aux schémas de niveau sonore.","(3) - Il s'agit d'une valeur relative qui varie en fonction de la distance et de l'environnement acoustique. Pour plus de détails, se reporter aux schémas de niveau sonore."]
["","","","","","(4) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(4) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(4) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]
["","","","","","(5) - Pour en savoir plus, se reporter au schéma de câblage, à la plaque signalétique et au manuel d'installation.","(5) - Pour en savoir plus, se reporter au schéma de câblage, à la plaque signalétique et au manuel d'installation.","(5) - Pour en savoir plus, se reporter au schéma de câblage, à la plaque signalétique et au manuel d'installation."]