{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Niveau de pression sonore","Chauffage","Haut","dBA","35","35","38","38"]
["","","Moyen","dBA","33","33","35","35"]
["","","Bas","dBA","27","27","30","30"]
["","Rafraîchissement","Moyen","dBA","33","33","35","35"]
["","","Bas","dBA","27","27","30","30"]
["","","Haut","dBA","35","35","38","38"]
["Accessoires standard","Manuel d'installation","","","1","1","1","1"]
["","Manuel d’utilisation","","","1","1","1","1"]
["","Isolant pour raccord","","","1","1","1","1"]
["","Tampon d’étanchéité","","","1","1","1","1"]
["","Attache métallique","","","1","1","1","1"]
["","Flexible d'évacuation","","","1","1","1","1"]
["","Rondelle pour attache de suspension","","","8","8","8","8"]
["","Matériau d'étanchéité","","","2","2","2","2"]
["","Attaches","","","6","6","6","6"]
["","Plaque de fixation à rondelle","","","4","4","4","4"]
["","Vis de brides à gaines","","","1","1","1","1"]
["","Filtre à air","","","1","1","1","1"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.50","9.50","12.70","12.70"]
["","Evacuation","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Puissance absorbée","Rafraîchissement","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Chauffage","Nom.","kW","0.036","0.036","0.060","0.060"]
["Sound power level","Rafraîchissement","","dBA","53","53","55","56"]
["","Chauffage","","dBA","53","53","55","56"]
["Dimensions","Unité","Largeur","mm","750","750","1,150","1,150"]
["","","Profondeur","mm","620","620","620","620"]
["","","Hauteur","mm","200","200","200","200"]
["Poids","Unité","","kg","21","21","28","28"]
["Ventilateur","Pression statique externe","Nom.","Pa","30","30","40","40"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Fréquence","","Hz","50","50","50","50"]
["","Tension","","V","220-240","220-240","220-240","220-240"]