{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25K3V1B","FDXS35F2VEB / RXS35K2V1B","FDXS50F2VEB / RXS50K2V1B"]
["Puissance frigorifique","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","3.0","3.8","5.3"]
["","Nom.","","kW","2.4 (2)","3.4 (2)","5.0 (2)"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5","12.7"]
["","Évacuation","OD","mm","VP20 (diamètre ext. : 26 / diamètre int. : 20)","VP20 (diamètre ext. : 26 / diamètre int. : 20)","VP20 (diamètre ext. : 26 / diamètre int. : 20)"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","323","530","825"]
["","EER","","","3.72 (1)","3.21 (1)","3.03 (1)"]
["","COP","","","3.90 (1)","3.39 (1)","3.10 (1)"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","B"]
["","","Chauffage","","A","C","D"]
["Puissance calorifique","Nom.","","kW","3.2 (3)","4.0 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","4.5","5.0","6.0"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m","(2) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m","(2) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m"]
["","","","","(3) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m","(3) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m","(3) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["","","","","(4) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(4) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(4) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]