{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Niveau de pression sonore","Chauffage","Haut","dBA","38"]
["","","Moyen","dBA","36"]
["","","Bas","dBA","30"]
["","Rafraîchissement","Moyen","dBA","36"]
["","","Bas","dBA","30"]
["","","Haut","dBA","38"]
["Accessoires standard","Manuel d'installation","","","1"]
["","Manuel d’utilisation","","","1"]
["","Isolant pour raccord","","","1"]
["","Tampon d’étanchéité","","","1"]
["","Attache métallique","","","1"]
["","Flexible d'évacuation","","","1"]
["","Rondelle pour attache de suspension","","","8"]
["","Matériau d'étanchéité","","","2"]
["","Attaches","","","6"]
["","Plaque de fixation à rondelle","","","4"]
["","Vis de brides à gaines","","","1"]
["","Filtre à air","","","1"]
["Piping connections","Liquide","DE","mm","6.35"]
["","Gaz","DE","mm","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Rafraîchissement","Nom.","kW","0.060"]
["","Chauffage","Nom.","kW","0.060"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","55"]
["","Chauffage","","dBA","55"]
["Dimensions","Unité","Largeur","mm","1,150"]
["","","Profondeur","mm","620"]
["","","Hauteur","mm","200"]
["Poids","Unité","","kg","30.0"]
["Ventilateur","Pression statique externe","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Fréquence","","Hz","50/60"]
["","Nom","","","VE"]
["","Tension","","V","220-240"]
["Remarques","","","","(1) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder."]