{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Puissance frigorifique","Nom.","","kW","","5.70"]
["Puissance calorifique","Nom.","","kW","","7.00"]
["Efficacité nominale","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Consommation énergétique annuelle","","kWh","","934"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","B"]
["","","Chauffage","","","B"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","","A+"]
["","Puissance","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Consommation d’énergie annuelle","","kWh/a","","347"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","A+"]
["","Puissance","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Consommation d’énergie annuelle","","kWh/a","","1,372"]
["Remarques","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(2) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","","(4) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["Unité extérieure","","","","RXM50N2V1B"]
["Puissance frigorifique","Nom.","","kW","5.00"]
["Puissance calorifique","Nom.","","kW","5.80"]
["Efficacité nominale","EER","","","3.24"]
["","COP","","","3.49"]
["","Consommation énergétique annuelle","","kWh","771"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","B"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+"]
["","Puissance","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["","Consommation d’énergie annuelle","","kWh/a","292"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A"]
["","Puissance","Pdesign","kW","3.84"]
["","SCOP/A","","","3.90"]
["","Pdh Puissance calorifique à -10°","","kW","3.51"]
["","Consommation d’énergie annuelle","","kWh/a","1377"]
["Classe d'efficacité énergétique","","","","A+++ ~ D"]