{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / RZASG71M2V1B","FHA71AVEB / RZASG71M2V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZASG100M7V1B","FHA50AVEB / FHA50AVEB / RZASG100M7V1B"]
["Puissance frigorifique","Nom.","","kW","6.80 (1)","6.80 (1)"]
["Rafraîchissement de l'air ambiant","SEER","","","7.33","5.95"]
["","Consommation d’énergie annuelle","","kWh/a","325","400"]
["","Puissance","Pdesign","kW","6.80","6.80"]
["","Classe d’efficacité énergétique","","","A++","A+"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","4.38","3.90"]
["","Classe d’efficacité énergétique","","","A+","A"]
["","Consommation d’énergie annuelle","","kWh/a","1,438","1,616"]
["Puissance calorifique","Nom.","","kW","7.50 (2)","7.50 (2)"]
["Remarques","","","","(1) - Rafraîchissement : T2 : temp. intérieure 26,6°C BS, 19,4°C BH ; temp. extérieure 48°C BS [Btu/h/W]","(1) - Rafraîchissement : T2 : temp. intérieure 26,6°C BS, 19,4°C BH ; temp. extérieure 48°C BS [Btu/h/W]","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["Outdoor unit","","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Puissance frigorifique","Nom.","","kW","","","9.50","9.50"]
["Puissance calorifique","Nom.","","kW","","","10.8","10.8"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","","","A++","A+"]
["","Puissance","Pdesign","kW","","","9.50","9.50"]
["","SEER","","","","","7.26","5.79"]
["","Consommation d’énergie annuelle","","kWh/a","","","458","574"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","","A+","A"]
["","Puissance","Pdesign","kW","","","6.00","6.00"]
["","SCOP/A","","","","","4.02","3.92"]
["","Consommation d’énergie annuelle","","kWh/a","","","2090","2143"]