{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Niveau de pression sonore","Chauffage","Haut","dBA","36","37","37","38"]
["","","Nom.","dBA","34","35","35","36"]
["","","Moyen","dBA","31","32","33","34"]
["","Rafraîchissement","Moyen","dBA","34","35","35","36"]
["","","Bas","dBA","31","32","33","34"]
["","","Haut","dBA","36","37","37","38"]
["Accessoires standard","Tube d'isolation thermique","","","2","2","2","2"]
["","Attache-câble","","","7","7","7","7"]
["","Collier de serrage","","","1","1","1","1"]
["","Flexible d'évacuation","","","1","1","1","1"]
["","Rondelle","","","8","8","8","8"]
["","Matériau d'étanchéité (grande taille)","","","1","1","1","1"]
["","Matériau d'étanchéité (petite taille)","","","1","1","1","1"]
["","Bague en résine","","","1","1","1","1"]
["","Vis","","","2","2","2","2"]
["","Dispositif de fixation de câbles","","","2","2","2","2"]
["Systèmes de contrôle","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35","9.52"]
["","Gaz","DE","mm","9.50","12.7","12.7","15.9"]
["","Evacuation","","","VP20","VP20","VP20","VP20"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","53","54","54","55"]
["Dimensions","Unité","Largeur","mm","960","960","1,270","1,270"]
["","","Profondeur","mm","690","690","690","690"]
["","","Hauteur","mm","235","235","235","235"]
["Caisson","Matériau","","","Résine, tôle","Résine, tôle","Résine, tôle","Résine, tôle"]
["","Couleur","","","Blanc","Blanc","Blanc","Blanc"]
["Poids","Unité","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Fréquence","","Hz","50","50","50","50"]
["","Tension","","V","220-240","220-240","220-240","220-240"]
["Remarques","","","","(1) - Pour les données électriques, se reporter au schéma séparé.","(1) - Pour les données électriques, se reporter au schéma séparé.","(1) - Pour les données électriques, se reporter au schéma séparé.","(1) - Pour les données électriques, se reporter au schéma séparé."]