{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Niveau de pression sonore","Chauffage","Haut","dBA","46"]
["","","Faible niveau sonore de fonctionnement","dBA","30"]
["","","Bas","dBA","33"]
["","Rafraîchissement","Faible niveau sonore de fonctionnement","dBA","29"]
["","","Bas","dBA","32"]
["","","Haut","dBA","38"]
["","","Nom.","dBA","36"]
["","Rafraîchissement","Nom.","dBA","35"]
["Accessoires standard","Manuel d'installation","","","1"]
["","Manuel d’utilisation","","","1"]
["","Télécommande infrarouge","","","1"]
["","Piles sèches AAA","","","2"]
["","Support de télécommande","","","1"]
["","Plaque de montage","","","1"]
["","Tube d'isolation thermique (tuyau de réfrigérant)","","","8"]
["","Filtre purificateur d'air","","","1"]
["","Filtre désodorisant photocatalytique","","","1"]
["","Couvercle latéral","","","2"]
["","Attache","","","4"]
["Systèmes de contrôle","Infrared remote control","","","ARC433B67"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35"]
["","Gaz","DE","mm","9.5"]
["","Evacuation","","","18"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","53"]
["","Chauffage","","dBA","59"]
["Dimensions","Unité","Largeur","mm","1,050"]
["","","Profondeur","mm","200"]
["","","Hauteur","mm","490"]
["Caisson","Couleur","","","Blanc amande"]
["Poids","Unité","","kg","16"]
["Power supply","Phase","","","1~"]
["","Fréquence","","Hz","50"]
["","Nom","","","VM"]
["","Tension","","V","220-240"]
["Remarques","","","","(1) - 220V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240V"]
["","","","","(4) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder."]