{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":14,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A"]
[]
[]
[]
[]
["","","","","","FTXF35A5V1B","FTXF50A2V1B","FTXF60A2V1B","FTXF71A2V1B","FTXF20A2V1B (Archived)","FTXF20A5V1B (Archived)","FTXF25A2V1B (Archived)","FTXF25A5V1B (Archived)","FTXF35A2V1B (Archived)"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","40","","","","39","39","40","40","40"]
["","","","Moyen","dBA","35","","","","34","34","34","34","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","","","","21","21","21","21","21"]
["","","","Bas","dBA","29","","","","28","28","28","28","29"]
["","Rafraîchissement","","Moyen","dBA","34","","","","33","33","33","33","34"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","","","","20","20","20","20","20"]
["","","","Bas","dBA","27","","","","25","25","26","26","27"]
["","","","Haut","dBA","43","","","","39","39","40","40","43"]
["Accessoires standard","Manuel d'installation","","","","1","","","","1","1","1","1","1"]
["","Manuel d’utilisation","","","","1","","","","1","1","1","1","1"]
["","Télécommande infrarouge","","","","1","","","","1","1","1","1","1"]
["","Piles sèches AAA","","","","2","","","","2","2","2","2","2"]
["","Support de télécommande","","","","1","","","","1","1","1","1","1"]
["","Plaque de montage","","","","1","","","","1","1","1","1","1"]
["","Vis de fixation d'unité intérieure","","","","2","","","","2","2","2","2","2"]
["Systèmes de contrôle","Wired remote control","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","","","","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.50","","","","9.50","9.50","9.50","9.50","9.50"]
["","Evacuation","","","","18","","","","18","18","18","18","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.032","","","","0.017","0.017","0.019","0.019","0.032"]
["","Chauffage","","Nom.","kW","0.032","","","","0.020","0.020","0.020","0.020","0.032"]
["Sound power level","Rafraîchissement","","","dBA","58","","","","55","55","55","55","58"]
["","Chauffage","","","dBA","58","","","","55","55","55","55","58"]
["Dimensions","Unité","","Largeur","mm","770","","","","770","770","770","770","770"]
["","","","Profondeur","mm","225","","","","225","225","225","225","225"]
["","","","Hauteur","mm","286","","","","286","286","286","286","286"]
["Caisson","Couleur","","","","Blanc","","","","Blanc","Blanc","Blanc","Blanc","Blanc"]
["Poids","Unité","","","kg","9.00","","","","9.00","9.00","9.00","9.00","9.00"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","11.5","","","","10.3","10.3","10.3","10.3","11.5"]
["","","","Bas","m³/min","7.0","","","","6.5","6.5","6.7","6.7","7.0"]
["","","","Moyen","m³/min","9.0","","","","8.4","8.4","8.6","8.6","9.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.3","","","","5.3","5.3","5.3","5.3","5.3"]
["","","Rafraîchissement","Bas","m³/min","6.3","","","","5.9","5.9","6.1","6.1","6.3"]
["","","","Moyen","m³/min","8.3","","","","7.9","7.9","8.1","8.1","8.3"]
["","","","Haut","m³/min","11.5","","","","9.8","9.8","10.1","10.1","11.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.5","","","","4.4","4.4","4.4","4.4","4.5"]
["Power supply","Phase","","","","1~","","","","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","","","","50","50","50","50","50"]
["","Tension","","","V","220-240","","","","220-240","220-240","220-240","220-240","220-240"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.029","0.032","0.032"]
["","Chauffage","","Nom.","kW","","0.032","0.035","0.035"]
["Caisson","Couleur","","","","","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","295","295","295"]
["","","","Largeur","mm","","990","990","990"]
["","","","Profondeur","mm","","263","263","263"]
["Poids","Unité","","","kg","","13.5","13.5","13.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","16.8","17.3","17.3"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","14.4","14.8","14.8"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","11.9","12.2","12.2"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","10.5","10.7","10.7"]
["","","Chauffage","Haut","m³/min","","17.3","17.9","17.9"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","14.8","15.8","15.8"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","12.2","12.8","12.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","10.7","11.3","11.3"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","59","60","62"]
["","Chauffage","","","dBA","","61","62","62"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","43","45","46"]
["","Refroidissement","","Moyen","dBA","","39","41","42"]
["","","","Bas","dBA","","34","36","37"]
["","","","Faible niveau sonore de fonctionnement","dBA","","31","33","34"]
["","Chauffage","","Haut","dBA","","42","44","45"]
["","","","Moyen","dBA","","38","40","41"]
["","","","Bas","dBA","","33","35","36"]
["","","","Faible niveau sonore de fonctionnement","dBA","","30","32","33"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35","6.35","6.35"]
["","Gaz","","DE","mm","","12.7","12.7","12.7"]
["","Évacuation","","","","","18","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Télécommande câblée","","","","","BRC073A1","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2"]
["","Operation manual","","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","2","2"]
["","Indoor unit fixing screws","","","","","2","2","2"]
["","Infrared remote control","","","","","1","1","1"]
["","Mounting plate","","","","","1","1","1"]
["","Remote control holder","","","","","1","1","1"]
["Alimentation électrique","Nom","","","","","V1","V1","V1"]
["","Phase","","","","","1~","1~","1~"]
["","Fréquence","","","Hz","","50","50","50"]
["","Tension","","","V","","220-240","220-240","220-240"]