{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Unité extérieure","","","","RXLG25M","RXLG35M"]
["Puissance frigorifique","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","2.5","3.5"]
["","Max.","","kW","4.0","4.6"]
["Puissance calorifique","Min.","","kW","1.0","1.0"]
["","Nom.","","kW","4.4","5.1"]
["","Max.","","kW","6.1, 3.6","6.7, 4.2"]
["Efficacité nominale","EER","","","3.68","3.57"]
["","COP","","","4.31","3.89"]
["","Consommation énergétique annuelle","","kWh","340","490"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Raccords de tuyauterie","Evacuation","DE","mm","18","18"]
["","Gaz","DE","mm","9.5","9.5"]
["","Liquide","DE","mm","6.35","6.35"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++","A++"]
["","Puissance","Pdesign","kW","2.50","3.50"]
["","SEER","","","7.04","6.67"]
["","Consommation d’énergie annuelle","","kWh/a","124","184"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A++","A++"]
["","Puissance","Pdesign","kW","2.50","3.00"]
["","SCOP/A","","","4.64","4.60"]
["","Consommation d’énergie annuelle","","kWh/a","755","913"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Pour puissance calorifique nominale minimale avec le ventilateur de l'unité intérieure réglé sur la position SL","(6) - Pour puissance calorifique nominale minimale avec le ventilateur de l'unité intérieure réglé sur la position SL"]
["","","","","(7) - Puissance calorifique maximale à -15 °C de température extérieure","(7) - Puissance calorifique maximale à -15 °C de température extérieure"]