{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B"]
["Puissance frigorifique","Nom.","","kW","4.00","","4.00","5.20","4.00","6.00"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","467","","471","593","457","787"]
["","EER","","","4.28","","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","","4.05","4.42","4.04","3.88"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","","A","A","A","A"]
["","","Chauffage","","A","","A","A","A","A"]
["Puissance calorifique","Nom.","","kW","4.60","","6.80","6.80","6.50","7.80"]
["Puissance frigorifique","Nom.","","kW","","4.00"]
["Puissance calorifique","Nom.","","kW","","4.60"]
["Efficacité nominale","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Consommation énergétique annuelle","","kWh","","482"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","A"]
["","","Chauffage","","","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","","A++"]
["","Puissance","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Consommation d’énergie annuelle","","kWh/a","","164"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","A+"]
["","Puissance","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh Puissance calorifique à -10°","","kW","","3.58"]
["","Consommation d’énergie annuelle","","kWh/a","","1632"]
["Remarques","","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(4) - Pour les données électriques, se reporter au schéma séparé."]