{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","","","41","46","47"]
["","","","Moyen","dBA","","","","38","42","43"]
["","","","Bas","dBA","","","","35","39","40"]
["","Rafraîchissement","","Moyen","dBA","","","","38","42","43"]
["","","","Bas","dBA","","","","35","39","40"]
["","","","Haut","dBA","","","","41","46","47"]
["Accessoires standard","Manuel d’utilisation","","","","","","","1","1","1"]
["","Manuel d'installation","","","","","","","1","1","1"]
["","Flexible d'évacuation","","","","","","","1","1","1"]
["","Tube d'isolation thermique","","","","","","","3","3","3"]
["","Attaches","","","","","","","10","10","10"]
["","Collier de serrage","","","","","","","1","1","1"]
["","Matériau d'étanchéité","","","","","","","4","4","4"]
["","Plaque de fixation à rondelle","","","","","","","1","1","1"]
["","Joint d'évacuation","","","","","","","1","1","1"]
["","Tissu non tissé","","","","","","","1","1","1"]
["","Rondelle","","","","","","","8","8","8"]
["","Vis de fixation pour flexible d'évacuation","","","","","","","5","5","5"]
["Systèmes de commande","Télécommande câblée","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","","","","","","12.1"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","","9.52","9.52","9.52"]
["","Gaz","","DE","mm","","","","15.9","15.9","15.9"]
["","Evacuation","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Rafraîchissement","","","dBA","","","","59","64","65"]
["","Chauffage","","","dBA","","","","59","64"]
["Dimensions","Unité","","Largeur","mm","","","","950","950","950"]
["","","","Profondeur","mm","","","","950","950","950"]
["","","","Hauteur","mm","","","","198","198","198"]
["Caisson","Matériau","","","","","","","Résine","Résine","Résine"]
["","Couleur","","","","","","","Blanc frais","Blanc frais","Blanc frais"]
["Poids","Unité","","","kg","","","","25.0","26.0","26"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","","","","23.0","31.0","32.5"]
["","","","Moyen","m³/min","","","","19.5","25.5","26.5"]
["","","","Bas","m³/min","","","","16.0","20.0","20.5"]
["","","Rafraîchissement","Bas","m³/min","","","","16.0","20.0","20.5"]
["","","","Moyen","m³/min","","","","19.5","25.5","26.5"]
["","","","Haut","m³/min","","","","23.0","31.0","32.5"]
["Hauteur manométrique","mm","","","","","","","600","600","600"]
["Puissance calorifique","Puissance totale","","Nom.","kW","","","","","","13.5"]
["Caisson","Couleur","","","","Blanc frais","Blanc frais","Blanc frais"]
["","Matériau","","","","Résine","Résine","Résine"]
["Dimensions","Unité","","Hauteur","mm","198","198","198"]
["","","","Largeur","mm","950","950","950"]
["","","","Profondeur","mm","950","950","950"]
["Poids","Unité","","","kg","25.0","26.0","26.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","23.0","31.0","32.5"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","19.5","25.5","26.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","16.0","20.0","20.5"]
["","","Chauffage","Haut","m³/min","23.0","31.0","32.5"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","19.5","25.5","26.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","16.0","20.0","20.5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","59","64","65"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","41","46","47"]
["","Refroidissement","","Moyen","dBA","38","42","43"]
["","","","Bas","dBA","35","39","40"]
["","Chauffage","","Haut","dBA","41","46","47"]
["","","","Moyen","dBA","38","42","43"]
["","","","Bas","dBA","35","39","40"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","9.52","9.52"]
["","Gaz","","DE","mm","15.9","15.9","15.9"]
["","Évacuation","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Hauteur manométrique","mm","","","","600","600","600"]
["Accessoires standard","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","","","12.10"]
["Puissance calorifique","Puissance totale","","Nom.","kW","","","13.5"]