{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L9V1B","FUQ71CVEB / RZQG71L9V1B","FUQ100CVEB / RZQG100L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG100L9V1B","FUQ125CVEB / RZQG125L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG125L9V1B"]
["Puissance frigorifique","Nom.","","kW","","6.8","9.5","","12.0"]
["Rafraîchissement de l'air ambiant","SEER","","","6.50","6.42","6.11","5.10","5.61","5.10"]
["","Consommation d’énergie annuelle","","kWh/a","367","371","545","652","749","824"]
["","Puissance","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Classe d’efficacité énergétique","","","A++","A++","A++","B","A+","B"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","7.60","7.60","11.30","11.30","14.13","12.71"]
["","SCOP/A","","","4.20","4.20","4.50","3.80","4.44","3.80"]
["","Classe d’efficacité énergétique","","","A+","A+","A+","A","A+","A"]
["","Consommation d’énergie annuelle","","kWh/a","2,534","2,534","3,516","4,164","4,456","4,683"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","840","1,230","","1,770"]
["","EER","","","","4.05","3.86","","3.39"]
["","COP","","","","4.08","3.95","","3.42"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","A","A","","A"]
["","","Chauffage","","","A","A","","B"]
["Puissance calorifique","Nom.","","kW","","7.5","10.8","","13.5"]
["Remarques","","","","","(1) - La consommation énergétique annuelle est conforme à la directive 2002/31/CE sur l'étiquetage énergétique.","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","","(2) - Les valeurs SEER et SCOP sont conformes à la norme EN 14825.","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]