{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZASG100M7Y1B","FVA125AMVEB / RZASG125M7Y1B","FVA140AMVEB / RZASG140M7Y1B","FVA71AMVEB / FVA71AMVEB / RZASG140M7Y1B"]
["Puissance frigorifique","Nom.","","kW","","12.1 (1)","13.4 (1)"]
["Rafraîchissement des locaux","Consommation d’énergie annuelle","","kWh/a","","1,314","1,428"]
["","Puissance","Pdesign","kW","","12.1","13.4"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","","6.00","7.80"]
["","Consommation d’énergie annuelle","","kWh/a","","2,308","2,866"]
["Puissance calorifique","Nom.","","kW","","13.5 (2)","15.5 (2)"]
["Puissance frigorifique","Nom.","","kW","9.5","","","13.4"]
["Puissance calorifique","Nom.","","kW","10.8","","","15.5"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+"]
["","Puissance","Pdesign","kW","9.5","","","13.4"]
["","SEER","","","5.72","","","7.71"]
["","Consommation d’énergie annuelle","","kWh/a","581","","","1043"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A"]
["","Puissance","Pdesign","kW","6","","","7.80"]
["","SCOP/A","","","3.83","","","4.43"]
["","Consommation d’énergie annuelle","","kWh/a","2193","","","2467"]
["Rafraîchissement des locaux","SEER","","","","5.52","5.63"]
["Chauffage des locaux (climat tempéré)","SCOP/A","","","","3.64","3.81"]
["Remarques","","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(4) - Pour les données électriques, se reporter au schéma séparé.","(4) - Pour les données électriques, se reporter au schéma séparé."]
["Classe d'efficacité énergétique","","","","","","","A+++ ~ D"]