{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-M"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25M2V1B","FVXG35K2V1B / RXLG35M2V1B"]
["Puissance frigorifique","Min.","","kW","1.2","1.4"]
["","Max.","","kW","5.1","5.6"]
["","Nom.","","kW","2.5 (2)","3.5 (2)"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5"]
["","Evacuation","DE","mm","18","18"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","355","510"]
["","EER","","","3.52 (1)","3.43 (1)"]
["","COP","","","3.88 (1)","3.61 (1)"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Puissance calorifique","Nom.","","kW","4.5 (2)","5.6 (2)"]
["","Min.","","kW","1.0 (6)","1.1 (6)"]
["","Max.","","kW","6.5, 3.5 (7)","7.0, 4.0 (7)"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Pour puissance calorifique nominale minimale avec le ventilateur de l'unité intérieure réglé sur la position SL","(6) - Pour puissance calorifique nominale minimale avec le ventilateur de l'unité intérieure réglé sur la position SL"]
["","","","","(7) - Puissance calorifique maximale à -15 °C de température extérieure","(7) - Puissance calorifique maximale à -15 °C de température extérieure"]