{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Type","","","","","Purificateur d'air"]
["Application","","","","","Type console carrossée"]
["Caisson","Colour","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","500"]
["","","","Largeur","mm","270"]
["","","","Profondeur","mm","270"]
["Poids","Unité","","","kg","6.8"]
["Surface applicable","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Fonctionnement en mode purification de l'air","Puissance absorbée","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","L","kW","0.010"]
["","","","Silence","kW","0.008"]
["Niveau de pression sonore","Fonctionnement en mode purification de l'air","","Turbo","dBA","53"]
["","","","Moyen","dBA","39"]
["","","","Bas","dBA","29"]
["","","","Silence","dBA","19"]
["Ventilateur","Débit d'air","Fonctionnement en mode purification de l'air","Turbo","m³/h","330"]
["","","","Moyen","m³/h","192"]
["","","","Bas","m³/h","120"]
["","","","Silence","m³/h","66"]
["Méthode de collecte des poussières","","","","","Filtre HEPA électrostatique"]
["Deodorizing method","","","","","Flash Streamer + catalyseur purificateur"]
["Dispositifs de sécurité","Élément","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Accessoires standard","Télécommande","","","","1"]
["","Support de télécommande","","","","1"]
["","Filtre HEPA électrostatique","","","","1"]
["","Filtre désodorisant","","","","1"]
["","Manuel d’utilisation","","","","1"]
["Cordon d'alimentation","m","","","","1.8"]
["Power supply","Phase","","","","1~"]
["","Fréquence","","","Hz","50/60"]
["","Tension","","","V","220-240/220-230"]
["Courant de fonctionnement","Fonctionnement en mode purification de l'air","","Turbo","A","0.32"]
["","","","Moyen","A","0.14"]
["","","","Bas","A","0.10"]
["","","","Silence","A","0.08"]
["Remarques","","","","","(1) - La surface applicable convient pour le fonctionnement de l’unité à la vitesse maximale du ventilateur (HH). La surface applicable fait référence à l'espace dans lequel une certaine quantité de particules de poussière peut être supprimée en 30 minutes. (JEM 1467)"]
["","","","","","(2) - Converti aux normes NRCC depuis les valeurs de test en conformité avec la norme JEM1467."]
["","","","","","(3) - Converti aux normes CADR depuis les valeurs de test en conformité avec la norme JEM1467."]
["","","","","","(4) - Les niveaux de pression sonore correspondent à la moyenne des valeurs mesurées à 1 m de distance de l'avant, des côtés gauche et droit, et du dessus de l'unité. (Ils sont égaux aux valeurs en chambre anéchoïde)"]
["","","","","","(5) - Le filtre HEPA électrostatique est fixé à l’unité."]
["","","","","","(6) - Autre fonction : Fonction de formage actif. Fonction de redémarrage automatique"]