{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC80Z"]
[]
[]
[]
[]
["","","","","","MC80ZVM"]
["Type","","","","","Purificateur d'air"]
["Application","","","","","Type console carrossée"]
["Caisson","Couleur","","","","Front: White, Top/Side: Dark Grey"]
["Dimensions","Unité","","Hauteur","mm","630"]
["","","","Largeur","mm","315"]
["","","","Profondeur","mm","315"]
["Poids","Unité","","","kg","9.8"]
["Surface applicable","m²","","","","62, 124"]
["CADR","m³/h","","","","480"]
["Mode purification","Puissance absorbée","","Turbo","kW","0.080"]
["","","","M","kW","0.016"]
["","","","L","kW","0.011"]
["","","","Silence","kW","0.009"]
["Niveau de pression sonore","Fonctionnement en mode purification de l'air","","Turbo","dBA","55"]
["","","","Moyen","dBA","34"]
["","","","Bas","dBA","25"]
["","","","Silence","dBA","19"]
["Ventilateur","Débit d'air","Fonctionnement en mode purification de l'air","Turbo","m³/h","480"]
["","","","Moyen","m³/h","210"]
["","","","Bas","m³/h","132"]
["","","","Silence","m³/h","84"]
["Méthode de collecte des poussières","","","","","Filtre HEPA électrostatique"]
["Méthode de désodorisation","","","","","Twin Streamer + Catalyseur désodorisant"]
["Accessoires standard","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["Cordon d'alimentation","m","","","","2"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50/60"]
["","Tension","","","V","220-240/220-230"]
["Remarques","","","","","(1) - La zone de couverture est appropriée pour un fonctionnement de l'unité à vitesse max. de ventilation (HH). La zone de couverture fait référence à l'espace dans lequel une certaine quantité de particules de poussière peut être supprimée en 30 minutes."]
["","","","","","(2) - Converti aux normes NRCC depuis les valeurs de test en conformité avec la norme JEM1467."]