{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-E"]
[]
[]
[]
[]
["","","","","","RXF20E5V1B","RXF25E5V1B","RXF35E5V1B","RXF42E5V1B"]
["Dimensions","Unité","","Hauteur","mm","556","556","556","556"]
["","","","Largeur","mm","740","740","740","740"]
["","","","Profondeur","mm","343","343","343","343"]
["Poids","Unité","","","kg","24.0","24.0","24.0","28.0"]
["Compresseur","Type","","","","Compresseur swing hermétique","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ambiante","Min.","°CBS","-10","-10","-10","-10"]
["","","","Max.","°CBS","48","48","48","48"]
["","Chauffage","Temp. ambiante","Min.","°CBH","-15","-15","-15","-15"]
["","","","Max.","°CBH","18","18","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46.0","46.0","48.0","48.0"]
["","Chauffage","","Haut","dBA","47.0","47.0","48.0","48.0"]
["Réfrigérant","Type","","","","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.420","0.420","0.550","0.750"]
["","Charge","","","tCO2Eq","0.280","0.280","0.370","0.510"]
["","PRP","","","","675.0","675.0","675.0","675.0"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20","20","20","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","12.0","12.0","12.0","12.0"]
["Accessoires standard","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50"]
["","Tension","","","V","220-240","220-240","220-240","220-240"]
["Compresseur","Type","","","","","Compresseur swing hermétique"]